Generating detailed summary of the adapter, it may take a while to complete.

CLI Version = 007.1324.0000.0000 June 1, 2020
Operating system = Windows Server 2016
Controller = 0
Status = Success
Description = None


Basics :
======
Controller = 0
Model = RAID 930-24i 4GB Flash
Serial Number = SXXXXXXX5
Current Controller Date/Time = 03/10/2022, 08:12:41
Current System Date/time = 03/10/2022, 08:12:43
SAS Address = 500062b1002dd100
PCI Address = 00:86:00:00
Mfg Date = 11/13/17
Rework Date = 00/00/00
Revision No = 26005


Version :
=======
Firmware Package Build = 50.0.1-0374
Firmware Version = 5.001.00-0805
CPLD Version = 05664-021
SBR Version = 260
Boot Block Version = 7.02.00.00-0015
Bios Version = 7.00.09.0_4.17.08.00_0x07001600
NVDATA Version = 4.1610.00-0093
Driver Name = megasas35.sys
Driver Version = 7.705.08.00


Bus :
===
Vendor Id = 0x1000
Device Id = 0x16
SubVendor Id = 0x1D49
SubDevice Id = 0x603
Host Interface = PCI-E
Device Interface = SAS-12G
Bus Number = 134
Device Number = 0
Function Number = 0
Domain ID = 0


Pending Images in Flash :
=======================
Image name = No pending images


Status :
======
Controller Status = Optimal
Memory Correctable Errors = 0
Memory Uncorrectable Errors = 0
ECC Bucket Count = 0
Any Offline VD Cache Preserved = No
BBU Status = 0
PD Firmware Download in progress = No
Support PD Firmware Download = Yes
Lock Key Assigned = No
Failed to get lock key on bootup = No
Lock key has not been backed up = No
Bios was not detected during boot = No
Controller must be rebooted to complete security operation = No
A rollback operation is in progress = No
At least one PFK exists in NVRAM = No
SSC Policy is WB = No
Controller has booted into safe mode = No
Controller shutdown required = No


Supported Adapter Operations :
============================
Rebuild Rate = Yes
CC Rate = Yes
BGI Rate  = Yes
Reconstruct Rate = Yes
Patrol Read Rate = Yes
Alarm Control = No
Cluster Support = No
BBU = Yes
Spanning = Yes
Dedicated Hot Spare = Yes
Revertible Hot Spares = Yes
Foreign Config Import = Yes
Self Diagnostic = Yes
Allow Mixed Redundancy on Array = No
Global Hot Spares = Yes
Deny SCSI Passthrough = No
Deny SMP Passthrough = No
Deny STP Passthrough = No
Support more than 8 Phys = Yes
FW and Event Time in GMT = No
Support Enhanced Foreign Import = Yes
Support Enclosure Enumeration = Yes
Support Allowed Operations = Yes
Abort CC on Error = Yes
Support Multipath = Yes
Support Odd & Even Drive count in RAID1E = No
Support Security = Yes
Support Config Page Model = Yes
Support the OCE without adding drives = Yes
Support EKM = Yes
Snapshot Enabled = No
Support PFK = Yes
Support PI = Yes
Support LDPI Type1 = No
Support LDPI Type2 = No
Support LDPI Type3 = No
Support Ld BBM Info = No
Support Shield State = Yes
Block SSD Write Disk Cache Change = Yes
Support Suspend Resume BG ops = Yes
Support Emergency Spares = Yes
Support Set Link Speed = Yes
Support Boot Time PFK Change = Yes
Support JBOD = Yes
Disable Online PFK Change = Yes
Support Perf Tuning = Yes
Support SSD PatrolRead = Yes
Real Time Scheduler = Yes
Support Reset Now = Yes
Support Emulated Drives = Yes
Headless Mode = Yes
Dedicated HotSpares Limited = No
Point In Time Progress = Yes
Extended LD = Yes
Support Uneven span  = No
Support Config Auto Balance = No
Support Maintenance Mode = No
Support Diagnostic results = Yes
Support Ext Enclosure = No
Support Sesmonitoring = Yes
Support SecurityonJBOD = Yes
Support ForceFlash = Yes
Support DisableImmediateIO = Yes
Support LargeIOSupport = No
Support DrvActivityLEDSetting = Yes
Support FlushWriteVerify = Yes
Support CPLDUpdate = Yes
Support ForceTo512e = Yes
Support discardCacheDuringLDDelete = No
Support JBOD Write cache = No
Support Large QD Support = No
Support Ctrl Info Extended = Yes
Support IButton less = Yes
Support AES Encryption Algorithm = No
Support Encrypted MFC = Yes
Support Snapdump = No
Support Force Personality Change = No
Support Dual Fw Image = No
Support PSOC Update = No
Support Secure Boot = No
Support Debug Queue = Yes
Support Least Latency Mode = Yes
Support OnDemand Snapdump = No
Support Clear Snapdump = No
Support PHY current speed = No
Support Lane current speed = No
Support NVMe Width = No
Support Lane DeviceType = No
Support Extended Drive performance Monitoring = No


Enterprise Key management :
=========================
Capability = Supported
Boot Agent = Available
Configured = No


Supported PD Operations :
=======================
Force Online = Yes
Force Offline = Yes
Force Rebuild = Yes
Deny Force Failed = No
Deny Force Good/Bad = No
Deny Missing Replace = No
Deny Clear = No
Deny Locate = No
Support Power State = No
Set Power State For Cfg = No
Support T10 Power State = No
Support Temperature = Yes
NCQ = Yes
Support Max Rate SATA = No
Support Degraded Media = No
Support Parallel FW Update = No
Support Drive Crypto Erase = No
Support SSD Wear Gauge = No


Supported VD Operations :
=======================
Read Policy = Yes
Write Policy = Yes
IO Policy = Yes
Access Policy = Yes
Disk Cache Policy = Yes
Reconstruction = Yes
Deny Locate = No
Deny CC = No
Allow Ctrl Encryption = No
Enable LDBBM = No
Support FastPath = Yes
Performance Metrics = Yes
Power Savings = No
Support Powersave Max With Cache = No
Support Breakmirror = Yes
Support SSC WriteBack = No
Support SSC Association = No
Support VD Hide = Yes
Support VD Cachebypass = Yes
Support VD discardCacheDuringLDDelete = No
Support VD Scsi Unmap = No


Advanced Software Option :
========================

-----------------------------------------
Adv S/W Opt         Time Remaining  Mode 
-----------------------------------------
MegaRAID FastPath   Unlimited       -    
MegaRAID SafeStore  Unlimited       -    
MegaRAID RAID6      Unlimited       -    
MegaRAID RAID5      Unlimited       -    
-----------------------------------------

Safe ID =  EQ3WU1IHBBI8L3V6GDNIX997S9G36M1NXE7T9URZ

HwCfg :
=====
ChipRevision =  B0
BatteryFRU = N/A
Front End Port Count = 0
Backend Port Count = 8
BBU = Present
Alarm = Missing
Serial Debugger = Present
NVRAM Size = 128KB
Flash Size = 16MB
On Board Memory Size = 4096MB
CacheVault Flash Size = 8.187 GB
TPM = Absent
Upgrade Key = Absent
On Board Expander = Absent
Temperature Sensor for ROC = Present
Temperature Sensor for Controller = Absent
Upgradable CPLD = Present
Upgradable PSOC = Absent
Current Size of CacheCade (GB) = 0
Current Size of FW Cache (MB) = 3183
ROC temperature(Degree Celsius) = 69


Policies :
========

Policies Table :
==============

------------------------------------------------
Policy                          Current Default 
------------------------------------------------
Predictive Fail Poll Interval   300 sec         
Interrupt Throttle Active Count 16              
Interrupt Throttle Completion   50 us           
Rebuild Rate                    30 %    30%     
PR Rate                         30 %    30%     
BGI Rate                        30 %    30%     
Check Consistency Rate          30 %    30%     
Reconstruction Rate             30 %    30%     
Cache Flush Interval            4s              
------------------------------------------------

Flush Time(Default) = 4s
Drive Coercion Mode = 1GB
Auto Rebuild = On
Battery Warning = On
ECC Bucket Size = 15
ECC Bucket Leak Rate (hrs) = 24
Restore Hot Spare on Insertion = Off
Expose Enclosure Devices = On
Maintain PD Fail History = On
Reorder Host Requests = On
Auto detect BackPlane = SGPIO/i2c SEP
Load Balance Mode = Auto
Security Key Assigned = Off
Disable Online Controller Reset = Off
Use drive activity for locate = Off


Boot :
====
BIOS Enumerate VDs = 1
Stop BIOS on Error = On
Delay during POST = 0
Spin Down Mode = None
Enable Ctrl-R = No
Enable Web BIOS = No
Enable PreBoot CLI = No
Enable BIOS = Yes
Max Drives to Spinup at One Time = 2
Maximum number of direct attached drives to spin up in 1 min = 60
Delay Among Spinup Groups (sec) = 2
Allow Boot with Preserved Cache = Off


High Availability :
=================
Topology Type = None
Cluster Permitted = No
Cluster Active = No


Defaults :
========
Phy Polarity = 0
Phy PolaritySplit = 0
Strip Size = 256 KB
Write Policy = WB
Read Policy = No Read Ahead
Cache When BBU Bad = Off
Cached IO = Off
VD PowerSave Policy = Controller Defined
Default spin down time (mins) = 30
Coercion Mode = 1 GB
ZCR Config = Unknown
Max Chained Enclosures = 3
Direct PD Mapping = No
Restore Hot Spare on Insertion = No
Expose Enclosure Devices = Yes
Maintain PD Fail History = Yes
Zero Based Enclosure Enumeration = No
Disable Puncturing = Yes
EnableLDBBM = No
DisableHII = No
Un-Certified Hard Disk Drives = Allow
SMART Mode = Mode 6
Enable LED Header = No
LED Show Drive Activity = Yes
Dirty LED Shows Drive Activity = No
EnableCrashDump = Yes
Disable Online Controller Reset = No
Treat Single span R1E as R10 = No
Power Saving option = Disabled
TTY Log In Flash = No
Auto Enhanced Import = Yes
BreakMirror RAID Support = single span R1
Disable Join Mirror = No
Enable Shield State = Yes
Time taken to detect CME = 60 sec


Capabilities :
============
Supported Drives = SAS, SATA
RAID Level Supported = RAID0, RAID1(2 or more drives), RAID5, RAID6, RAID00, RAID10(2 or more drives per span), RAID50, RAID60
Enable JBOD = No
Mix in Enclosure = Allowed
Mix of SAS/SATA of HDD type in VD = Not Allowed
Mix of SAS/SATA of SSD type in VD = Not Allowed
Mix of SSD/HDD in VD = Not Allowed
SAS Disable = No
Max Arms Per VD = 32
Max Spans Per VD = 8
Max Arrays = 128
Max VD per array = 64
Max Number of VDs = 64
Max Parallel Commands = 4077
Max SGE Count = 60
Max Data Transfer Size = 8192 sectors
Max Strips PerIO = 42
Max Configurable CacheCade Size(GB) = 0
Max Transportable DGs = 0
Enable Snapdump = No
Enable SCSI Unmap = Yes
FDE Drive Mix Support = No
Min Strip Size = 64 KB
Max Strip Size = 1.000 MB


Scheduled Tasks :
===============
Consistency Check Reoccurrence = 168 hrs
Next Consistency check launch = 03/12/2022, 03:00:00
Patrol Read Reoccurrence = 168 hrs
Next Patrol Read launch = 03/12/2022, 03:00:00
Battery learn Reoccurrence = 670 hrs
Next Battery Learn = 03/27/2022, 10:00:00
OEMID = Lenovo

Drive Groups = 2

TOPOLOGY :
========

------------------------------------------------------------------------------
DG Arr Row EID:Slot DID Type   State BT       Size PDC  PI SED DS3  FSpace TR 
------------------------------------------------------------------------------
 0 -   -   -        -   RAID1  Optl  N  893.137 GB dflt N  N   dflt N      N  
 0 0   -   -        -   RAID1  Optl  N  893.137 GB dflt N  N   dflt N      N  
 0 0   0   65:0     46  DRIVE  Onln  N  893.137 GB dflt N  N   dflt -      N  
 0 0   1   65:1     47  DRIVE  Onln  N  893.137 GB dflt N  N   dflt -      N  
 1 -   -   -        -   RAID10 Optl  N   10.904 TB dsbl N  N   dflt N      N  
 1 0   -   -        -   RAID1  Optl  N    2.180 TB dsbl N  N   dflt N      N  
 1 0   0   65:2     49  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 0   1   65:3     41  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 0   2   65:4     40  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 0   3   65:5     44  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 1   -   -        -   RAID1  Optl  N    2.180 TB dsbl N  N   dflt N      N  
 1 1   0   65:6     39  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 1   1   65:7     43  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 1   2   65:8     37  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 1   3   65:9     36  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 2   -   -        -   RAID1  Optl  N    2.180 TB dsbl N  N   dflt N      N  
 1 2   0   65:10    35  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 2   1   65:11    42  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 2   2   65:12    34  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 2   3   65:13    33  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 3   -   -        -   RAID1  Optl  N    2.180 TB dsbl N  N   dflt N      N  
 1 3   0   65:14    31  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 3   1   65:15    30  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 3   2   65:16    38  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 3   3   65:17    27  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 4   -   -        -   RAID1  Optl  N    2.180 TB dsbl N  N   dflt N      N  
 1 4   0   65:18    28  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 4   1   65:19    26  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 4   2   65:20    25  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 4   3   65:21    32  DRIVE  Onln  N    1.089 TB dsbl N  N   dflt -      N  
 1 -   -   65:23    29  DRIVE  DHS   -    1.089 TB -    -  -   -    -      N  
------------------------------------------------------------------------------

DG=Disk Group Index|Arr=Array Index|Row=Row Index|EID=Enclosure Device ID
DID=Device ID|Type=Drive Type|Onln=Online|Rbld=Rebuild|Optl=Optimal|Dgrd=Degraded
Pdgd=Partially degraded|Offln=Offline|BT=Background Task Active
PDC=PD Cache|PI=Protection Info|SED=Self Encrypting Drive|Frgn=Foreign
DS3=Dimmer Switch 3|dflt=Default|Msng=Missing|FSpace=Free Space Present
TR=Transport Ready

Virtual Drives = 2

VD LIST :
=======

-------------------------------------------------------------------
DG/VD TYPE   State Access Consist Cache Cac sCC       Size Name    
-------------------------------------------------------------------
0/0   RAID1  Optl  RW     Yes     RWBD  -   ON  893.137 GB OS      
1/1   RAID10 Optl  RW     Yes     RWBD  -   ON   10.904 TB Volume1 
-------------------------------------------------------------------

VD=Virtual Drive| DG=Drive Group|Rec=Recovery
Cac=CacheCade|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|dflt=Default|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
AWB=Always WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency

Physical Drives = 24

PD LIST :
=======

-----------------------------------------------------------------------------------------------------
EID:Slt DID State DG       Size Intf Med SED PI SeSz Model                                   Sp Type 
-----------------------------------------------------------------------------------------------------
65:0     46 Onln   0 893.137 GB SATA SSD N   N  512B MTFDDAK960TDC-1AT1ZA 01PE307D7A09592LEN U  -    
65:1     47 Onln   0 893.137 GB SATA SSD N   N  512B MTFDDAK960TDC-1AT1ZA 01PE307D7A09592LEN U  -    
65:2     49 Onln   1   1.089 TB SAS  HDD N   N  512B ST1200MM0009                            U  -    
65:3     41 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:4     40 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:5     44 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:6     39 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:7     43 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:8     37 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:9     36 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:10    35 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:11    42 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:12    34 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:13    33 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:14    31 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:15    30 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:16    38 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:17    27 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:18    28 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:19    26 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:20    25 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:21    32 Onln   1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
65:22    48 UGood  -   1.089 TB SAS  HDD N   N  512B ST1200MM0009                            U  -    
65:23    29 DHS    1   1.089 TB SAS  HDD N   N  512B AL15SEB120N                             U  -    
-----------------------------------------------------------------------------------------------------

EID=Enclosure Device ID|Slt=Slot No.|DID=Device ID|DG=DriveGroup
DHS=Dedicated Hot Spare|UGood=Unconfigured Good|GHS=Global Hotspare
UBad=Unconfigured Bad|Sntze=Sanitize|Onln=Online|Offln=Offline|Intf=Interface
Med=Media Type|SED=Self Encryptive Drive|PI=Protection Info
SeSz=Sector Size|Sp=Spun|U=Up|D=Down|T=Transition|F=Foreign
UGUnsp=UGood Unsupported|UGShld=UGood shielded|HSPShld=Hotspare shielded
CFShld=Configured shielded|Cpybck=CopyBack|CBShld=Copyback Shielded
UBUnsp=UBad Unsupported|Rbld=Rebuild

Enclosures = 2

Enclosure LIST :
==============

-----------------------------------------------------------------------
EID State Slots PD PS Fans TSs Alms SIM Port# ProdID    VendorSpecific 
-----------------------------------------------------------------------
 65 OK       24 24  0    0   0    0   0       SAS35x36R exp-0.3.2.0    
134 OK        8  0  0    0   0    0   1 -     SGPIO                    
-----------------------------------------------------------------------

EID=Enclosure Device ID |PD=Physical drive count |PS=Power Supply count|
TSs=Temperature sensor count |Alms=Alarm count |SIM=SIM Count ||ProdID=Product ID


Cachevault_Info :
===============

------------------------------------
Model  State   Temp Mode MfgDate    
------------------------------------
CVPM02 Optimal 29C  -    2018/04/05 
------------------------------------
