Generating detailed summary of the adapter, it may take a while to complete.

CLI Version = 007.0529.0000.0000 Sep 18, 2018
Operating system = Linux 4.9.0-18-amd64
Controller = 0
Status = Success
Description = None


Basics :
======
Controller = 0
Model = PERC H730P Adapter
Serial Number = 8BN01234
Current Controller Date/Time = 06/27/2022, 21:30:40
Current System Date/time = 06/27/2022, 23:30:42
SAS Address = 54cdabf010303400
PCI Address = 00:18:00:00
Mfg Date = 11/27/18
Rework Date = 11/27/18
Revision No = A04


Version :
=======
Firmware Package Build = 25.5.5.0005
Firmware Version = 4.290.00-8334
Bios Version = 6.33.01.0_4.16.07.00_0x06120304
Ctrl-R Version = 5.18-0701
NVDATA Version = 3.1511.00-0028
Boot Block Version = 3.07.00.00-0003
Driver Name = megaraid_sas
Driver Version = 07.700.00.00-rc1


Bus :
===
Vendor Id = 0x1000
Device Id = 0x5D
SubVendor Id = 0x1028
SubDevice Id = 0x1F42
Host Interface = PCI-E
Device Interface = SAS-12G
Bus Number = 24
Device Number = 0
Function Number = 0


Pending Images in Flash :
=======================
Image name = No pending images


Status :
======
Controller Status = Optimal
Memory Correctable Errors = 0
Memory Uncorrectable Errors = 0
ECC Bucket Count = 0
Any Offline VD Cache Preserved = No
BBU Status = 0
PD Firmware Download in progress = No
Lock Key Assigned = No
Failed to get lock key on bootup = No
Lock key has not been backed up = No
Bios was not detected during boot = No
Controller must be rebooted to complete security operation = No
A rollback operation is in progress = No
At least one PFK exists in NVRAM = No
SSC Policy is WB = No
Controller has booted into safe mode = No
Current Personality = RAID-Mode 


Supported Adapter Operations :
============================
Rebuild Rate = Yes
CC Rate = Yes
BGI Rate  = Yes
Reconstruct Rate = Yes
Patrol Read Rate = Yes
Alarm Control = Yes
Cluster Support = No
BBU  = Yes
Spanning = Yes
Dedicated Hot Spare = Yes
Revertible Hot Spares = Yes
Foreign Config Import = Yes
Self Diagnostic = Yes
Allow Mixed Redundancy on Array = No
Global Hot Spares = Yes
Deny SCSI Passthrough = No
Deny SMP Passthrough = No
Deny STP Passthrough = No
Support more than 8 Phys = Yes
FW and Event Time in GMT = No
Support Enhanced Foreign Import = Yes
Support Enclosure Enumeration = Yes
Support Allowed Operations = Yes
Abort CC on Error = Yes
Support Multipath = Yes
Support Odd & Even Drive count in RAID1E = No
Support Security = Yes
Support Config Page Model = Yes
Support the OCE without adding drives = Yes
Support EKM = No
Snapshot Enabled = No
Support PFK = No
Support PI = No
Support Ld BBM Info = No
Support Shield State = Yes
Block SSD Write Disk Cache Change = No
Support Suspend Resume BG ops = Yes
Support Emergency Spares = No
Support Set Link Speed = Yes
Support Boot Time PFK Change = No
Support SystemPD = Yes
Disable Online PFK Change = No
Support Perf Tuning = Yes
Support SSD PatrolRead = Yes
Real Time Scheduler = No
Support Reset Now = Yes
Support Emulated Drives = Yes
Headless Mode = Yes
Dedicated HotSpares Limited = No
Point In Time Progress = No
Extended LD = Yes
Boot Volume Supported = No
Support Uneven span  = Yes
Support Config Auto Balance = No
Support Maintenance Mode = No
Support Diagnostic results = Yes
Support Ext Enclosure = No
Support Sesmonitoring = No
Support SecurityonJBOD = No
Support ForceFlash = No
Support DisableImmediateIO = No
Support LargeIOSupport = Yes
Support DrvActivityLEDSetting = No
Support FlushWriteVerify = No
Support CPLDUpdate = No
Support ForceTo512e = No
Support discardCacheDuringLDDelete = No
Support JBOD Write cache = Yes
Support Large QD Support = No
Support Ctrl Info Extended = No
Support IButton less = No
Support AES Encryption Algorithm = No
Support Encrypted MFC = No
Support Force Personality Change = No


Enterprise Key management :
=========================
Capability = Not Supported


Supported PD Operations :
=======================
Force Online = Yes
Force Offline = Yes
Force Rebuild = Yes
Deny Force Failed = No
Deny Force Good/Bad = No
Deny Missing Replace = No
Deny Clear = No
Deny Locate = No
Support Power State = Yes
Set Power State For Cfg = No
Support T10 Power State = Yes
Support Temperature = Yes
NCQ = No
Support Max Rate SATA = No
Support Degraded Media = No
Support Parallel FW Update = No
Support Drive Crypto Erase = Yes


Supported VD Operations :
=======================
Read Policy = Yes
Write Policy = Yes
IO Policy = Yes
Access Policy = Yes
Disk Cache Policy = Yes
Reconstruction = Yes
Deny Locate = No
Deny CC = No
Allow Ctrl Encryption = No
Enable LDBBM = Yes
Support FastPath = Yes
Performance Metrics = Yes
Power Savings = Yes
Support Powersave Max With Cache = No
Support Breakmirror = Yes
Support SSC WriteBack = No
Support SSC Association = No
Support VD Hide = No
Support VD Cachebypass = Yes
Support VD discardCacheDuringLDDelete = No
Support VD Scsi Unmap = No


HwCfg :
=====
ChipRevision =  C0
BatteryFRU = N/A
Front End Port Count = 0
Backend Port Count = 8
BBU = Present
Alarm = Missing
Serial Debugger = Present
NVRAM Size = 32KB
Flash Size = 16MB
On Board Memory Size = 2048MB
CacheVault Flash Size = 4.0 GB
TPM = Absent
Upgrade Key = Absent
On Board Expander = Absent
Temperature Sensor for ROC = Present
Temperature Sensor for Controller = Present
Upgradable CPLD = Absent
Current Size of CacheCade (GB) = 0
Current Size of FW Cache (MB) = 1931
ROC temperature(Degree Celsius) = 56
Ctrl temperature(Degree Celsius) = 56


Policies :
========

Policies Table :
==============

------------------------------------------------
Policy                          Current Default 
------------------------------------------------
Predictive Fail Poll Interval   300 sec         
Interrupt Throttle Active Count 16              
Interrupt Throttle Completion   50 us           
Rebuild Rate                    30 %    30%     
PR Rate                         30 %    30%     
BGI Rate                        30 %    30%     
Check Consistency Rate          30 %    30%     
Reconstruction Rate             30 %    30%     
Cache Flush Interval            4s              
------------------------------------------------

Flush Time(Default) = 4s
Drive Coercion Mode = 128MB
Auto Rebuild = On
Battery Warning = On
ECC Bucket Size = 255
ECC Bucket Leak Rate (hrs) = 4
Restore HotSpare on Insertion = Off
Expose Enclosure Devices = Off
Maintain PD Fail History = Off
Reorder Host Requests = On
Auto detect BackPlane = SGPIO/i2c SEP
Load Balance Mode = Auto
Security Key Assigned = Off
Disable Online Controller Reset = Off
Use drive activity for locate = Off


Boot :
====
BIOS Enumerate VDs = 1
Stop BIOS on Error = Off
Delay during POST = 0
Spin Down Mode = None
Enable Ctrl-R = Yes
Enable Web BIOS = No
Enable PreBoot CLI = No
Enable BIOS = Yes
Max Drives to Spinup at One Time = 4
Maximum number of direct attached drives to spin up in 1 min = 0
Delay Among Spinup Groups (sec) = 12
Allow Boot with Preserved Cache = Off


High Availability :
=================
Topology Type = None
Cluster Permitted = No
Cluster Active = No


Defaults :
========
Phy Polarity = 0
Phy PolaritySplit = 0
Strip Size = 64 KB
Write Policy = WB
Read Policy = Adaptive
Cache When BBU Bad = Off
Cached IO = Off
VD PowerSave Policy = Controller Defined
Default spin down time (mins) = 30
Coercion Mode = 128 MB
ZCR Config = Unknown
Max Chained Enclosures = 4
Direct PD Mapping = Yes
Restore Hot Spare on Insertion = No
Expose Enclosure Devices = No
Maintain PD Fail History = No
Zero Based Enclosure Enumeration = Yes
Disable Puncturing = No
EnableLDBBM = Yes
DisableHII = No
Un-Certified Hard Disk Drives = Allow
SMART Mode = Mode 6
Enable LED Header = No
LED Show Drive Activity = Yes
Dirty LED Shows Drive Activity = No
EnableCrashDump = No
Disable Online Controller Reset = No
Treat Single span R1E as R10 = Yes
Power Saving option = Enabled
TTY Log In Flash = Yes
Auto Enhanced Import = No
BreakMirror RAID Support = Yes
Disable Join Mirror = Yes
Enable Shield State = No
Time taken to detect CME = 60 sec


Capabilities :
============
Supported Drives = SAS, SATA
Boot Volume Supported = NO
RAID Level Supported = RAID0, RAID1, RAID5, RAID6, RAID10(2 or more drives per span), RAID50, RAID60
Enable SystemPD = Yes
Mix in Enclosure = Allowed
Mix of SAS/SATA of HDD type in VD = Not Allowed
Mix of SAS/SATA of SSD type in VD = Not Allowed
Mix of SSD/HDD in VD = Not Allowed
SAS Disable = No
Max Arms Per VD = 32
Max Spans Per VD = 8
Max Arrays = 128
Max VD per array = 16
Max Number of VDs = 64
Max Parallel Commands = 928
Max SGE Count = 60
Max Data Transfer Size = 8192 sectors
Max Strips PerIO = 128
Max Configurable CacheCade Size(GB) = 0
Max Transportable DGs = 0
Min Strip Size = 64 KB
Max Strip Size = 1.0 MB


Scheduled Tasks :
===============
Consistency Check Reoccurrence = 168 hrs
Next Consistency check launch = NA
Patrol Read Reoccurrence = 168 hrs
Next Patrol Read launch = 07/02/2022, 03:00:00
Battery learn Reoccurrence = 2160 hrs
OEMID = Dell

Drive Groups = 2

TOPOLOGY :
========

-----------------------------------------------------------------------------
DG Arr Row EID:Slot DID Type  State BT       Size PDC  PI SED DS3  FSpace TR 
-----------------------------------------------------------------------------
 0 -   -   -        -   RAID1 Optl  N  744.625 GB dflt N  N   dflt N      N  
 0 0   -   -        -   RAID1 Optl  N  744.625 GB dflt N  N   dflt N      N  
 0 0   0   32:0     0   DRIVE Onln  N  744.625 GB dflt N  N   dflt -      N  
 0 0   1   32:1     1   DRIVE Onln  N  744.625 GB dflt N  N   dflt -      N  
 1 -   -   -        -   RAID5 Optl  N    2.727 TB dflt N  N   dflt N      N  
 1 0   -   -        -   RAID5 Optl  N    2.727 TB dflt N  N   dflt N      N  
 1 0   0   32:2     2   DRIVE Onln  N    931.0 GB dflt N  N   dflt -      N  
 1 0   1   32:3     3   DRIVE Onln  N    931.0 GB dflt N  N   dflt -      N  
 1 0   2   32:4     4   DRIVE Onln  N    931.0 GB dflt N  N   dflt -      N  
 1 0   3   32:5     5   DRIVE Onln  N    931.0 GB dflt N  N   dflt -      N  
-----------------------------------------------------------------------------

DG=Disk Group Index|Arr=Array Index|Row=Row Index|EID=Enclosure Device ID
DID=Device ID|Type=Drive Type|Onln=Online|Rbld=Rebuild|Dgrd=Degraded
Pdgd=Partially degraded|Offln=Offline|BT=Background Task Active
PDC=PD Cache|PI=Protection Info|SED=Self Encrypting Drive|Frgn=Foreign
DS3=Dimmer Switch 3|dflt=Default|Msng=Missing|FSpace=Free Space Present
TR=Transport Ready

Virtual Drives = 2

VD LIST :
=======

-------------------------------------------------------------------------
DG/VD TYPE  State Access Consist Cache Cac sCC       Size Name           
-------------------------------------------------------------------------
0/0   RAID1 Optl  RW     Yes     RWBD  -   OFF 744.625 GB Virtual Disk 0 
1/1   RAID5 Optl  RW     Yes     RWBD  -   OFF   2.727 TB Virtual Disk 1 
-------------------------------------------------------------------------

Cac=CacheCade|Rec=Recovery|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
FWB=Force WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency

Physical Drives = 6

PD LIST :
=======

---------------------------------------------------------------------------
EID:Slt DID State DG       Size Intf Med SED PI SeSz Model         Sp Type 
---------------------------------------------------------------------------
32:0      0 Onln   0 744.625 GB SATA SSD N   N  512B SSDSC2BB800G7 U  -    
32:1      1 Onln   0 744.625 GB SATA SSD N   N  512B SSDSC2BB800G7 U  -    
32:2      2 Onln   1   931.0 GB SATA HDD N   N  512B ST1000NX0443  U  -    
32:3      3 Onln   1   931.0 GB SATA HDD N   N  512B ST1000NX0443  U  -    
32:4      4 Onln   1   931.0 GB SATA HDD N   N  512B ST1000NX0443  U  -    
32:5      5 Onln   1   931.0 GB SATA HDD N   N  512B ST1000NX0443  U  -    
---------------------------------------------------------------------------

EID-Enclosure Device ID|Slt-Slot No.|DID-Device ID|DG-DriveGroup
DHS-Dedicated Hot Spare|UGood-Unconfigured Good|GHS-Global Hotspare
UBad-Unconfigured Bad|Onln-Online|Offln-Offline|Intf-Interface
Med-Media Type|SED-Self Encrypting Drive|PI-Protection Info
SeSz-Sector Size|Sp-Spun|U-Up|D-Down/PowerSave|T-Transition|F-Foreign
UGUnsp-Unsupported|UGShld-UnConfigured shielded|HSPShld-Hotspare shielded
CFShld-Configured shielded|Cpybck-CopyBack|CBShld-Copyback Shielded


BBU_Info :
========

----------------------------------------------
Model State   RetentionTime Temp Mode MfgDate 
----------------------------------------------
BBU   Optimal 0 hour(s)     25C  -    0/00/00 
----------------------------------------------



CLI Version = 007.0529.0000.0000 Sep 18, 2018
Operating system = Linux 4.9.0-18-amd64
Controller = 0
Status = Success
Description = None


/c0/v0 :
======

-------------------------------------------------------------------------
DG/VD TYPE  State Access Consist Cache Cac sCC       Size Name           
-------------------------------------------------------------------------
0/0   RAID1 Optl  RW     Yes     RWBD  -   OFF 744.625 GB Virtual Disk 0 
-------------------------------------------------------------------------

Cac=CacheCade|Rec=Recovery|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
FWB=Force WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency


PDs for VD 0 :
============

---------------------------------------------------------------------------
EID:Slt DID State DG       Size Intf Med SED PI SeSz Model         Sp Type 
---------------------------------------------------------------------------
32:0      0 Onln   0 744.625 GB SATA SSD N   N  512B THNSF8800CCSE U  -    
32:1      1 Onln   0 744.625 GB SATA SSD N   N  512B THNSF8800CCSE U  -    
---------------------------------------------------------------------------

EID-Enclosure Device ID|Slt-Slot No.|DID-Device ID|DG-DriveGroup
DHS-Dedicated Hot Spare|UGood-Unconfigured Good|GHS-Global Hotspare
UBad-Unconfigured Bad|Onln-Online|Offln-Offline|Intf-Interface
Med-Media Type|SED-Self Encrypting Drive|PI-Protection Info
SeSz-Sector Size|Sp-Spun|U-Up|D-Down/PowerSave|T-Transition|F-Foreign
UGUnsp-Unsupported|UGShld-UnConfigured shielded|HSPShld-Hotspare shielded
CFShld-Configured shielded|Cpybck-CopyBack|CBShld-Copyback Shielded


VD0 Properties :
==============
Strip Size = 64 KB
Number of Blocks = 1561591808
VD has Emulated PD = No
Span Depth = 1
Number of Drives Per Span = 2
Write Cache(initial setting) = WriteBack
Disk Cache Policy = Disk's Default
Encryption = None
Data Protection = None
Active Operations = None
Exposed to OS = Yes
Creation Date = 04-01-2019
Creation Time = 11:04:16 PM
Emulation type = default
Cachebypass size = Cachebypass-64k
Cachebypass Mode = Cachebypass Intelligent
Is LD Ready for OS Requests = Yes
SCSI NAA Id = 64cd98f040f0fd0023c2a2f070eefd16
SCSI Unmap = No


/c0/v1 :
======

-----------------------------------------------------------------------
DG/VD TYPE  State Access Consist Cache Cac sCC     Size Name           
-----------------------------------------------------------------------
1/1   RAID5 Optl  RW     Yes     RWBD  -   OFF 2.727 TB Virtual Disk 1 
-----------------------------------------------------------------------

Cac=CacheCade|Rec=Recovery|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
FWB=Force WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency


PDs for VD 1 :
============

------------------------------------------------------------------------
EID:Slt DID State DG     Size Intf Med SED PI SeSz Model        Sp Type 
------------------------------------------------------------------------
32:2      2 Onln   1 931.0 GB SATA HDD N   N  512B ST1000NX0443 U  -    
32:3      3 Onln   1 931.0 GB SATA HDD N   N  512B ST1000NX0443 U  -    
32:4      4 Onln   1 931.0 GB SATA HDD N   N  512B ST1000NX0443 U  -    
32:5      5 Onln   1 931.0 GB SATA HDD N   N  512B ST1000NX0443 U  -    
------------------------------------------------------------------------

EID-Enclosure Device ID|Slt-Slot No.|DID-Device ID|DG-DriveGroup
DHS-Dedicated Hot Spare|UGood-Unconfigured Good|GHS-Global Hotspare
UBad-Unconfigured Bad|Onln-Online|Offln-Offline|Intf-Interface
Med-Media Type|SED-Self Encrypting Drive|PI-Protection Info
SeSz-Sector Size|Sp-Spun|U-Up|D-Down/PowerSave|T-Transition|F-Foreign
UGUnsp-Unsupported|UGShld-UnConfigured shielded|HSPShld-Hotspare shielded
CFShld-Configured shielded|Cpybck-CopyBack|CBShld-Copyback Shielded


VD1 Properties :
==============
Strip Size = 64 KB
Number of Blocks = 5857345536
VD has Emulated PD = No
Span Depth = 1
Number of Drives Per Span = 4
Write Cache(initial setting) = WriteBack
Disk Cache Policy = Disk's Default
Encryption = None
Data Protection = None
Active Operations = None
Exposed to OS = Yes
Creation Date = 04-01-2019
Creation Time = 11:04:44 PM
Emulation type = default
Cachebypass size = Cachebypass-64k
Cachebypass Mode = Cachebypass Intelligent
Is LD Ready for OS Requests = Yes
SCSI NAA Id = 64cd98f040f0fd0023c2a30c729a1fb9
SCSI Unmap = No



