Sensor ID              : BIOS (0x0)
 Entity ID             : 0.0
 Sensor Type (Discrete): System Firmwares
 Unable to read sensor: Device Not Present

Sensor ID              : ACPI State (0x20)
 Entity ID             : 0.0
 Sensor Type (Discrete): System ACPI Power State
 States Asserted       : System ACPI Power State
                         [S0/G0: working]

Sensor ID              : System Reset (0x21)
 Entity ID             : 0.0
 Sensor Type (Discrete): Module / Board

Sensor ID              : CPU Fan (0x31)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Fan
 Sensor Reading        : 2085.941 (+/- inf) RPM
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 771.962
 Upper Non-Recoverable : na
 Positive Hysteresis   : 39215.686
 Negative Hysteresis   : 39215.686
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr+ 

Sensor ID              : Rear Fan (0x34)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Fan
 Sensor Reading        : 1463.272 (+/- inf) RPM
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 771.962
 Upper Non-Recoverable : na
 Positive Hysteresis   : 39215.686
 Negative Hysteresis   : 39215.686
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr+ 

Sensor ID              : System 12V (0x41)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 11.928 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 10.024
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 13.160
 Upper Non-Recoverable : na
 Positive Hysteresis   : 0.280
 Negative Hysteresis   : 0.280
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : System 5V (0x36)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 5.054 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 4.750
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 5.242
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : System AUX 5V (0x37)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 4.937 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 4.750
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 5.242
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : System 3.3V (0x38)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 3.219 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 3.142
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 3.465
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : System AUX 3.3V (0x39)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 3.311 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 3.142
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 3.465
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : CPU Vcore (0x3a)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 1.284 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 0.843
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 1.607
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : CPU Vterm (0x3c)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 1.196 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 1.147
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 1.264
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : Memory Vcore (0x3d)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 1.784 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 1.705
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 1.911
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : Memory Vterm (0x3e)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 0.882 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 0.853
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 0.941
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : AMB/MCH Vcore (0x3f)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Voltage
 Sensor Reading        : 1.499 (+/- 0) Volts
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : 1.431
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 1.578
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : lcr- ucr+ 
 Deassertions Enabled  : lcr- ucr+ 

Sensor ID              : PCI System Err (0x42)
 Entity ID             : 0.0
 Sensor Type (Discrete): Module / Board
 Unable to read sensor: Device Not Present

Sensor ID              : Mem Recover Err (0x44)
 Entity ID             : 0.0
 Sensor Type (Discrete): Memory
 Unable to read sensor: Device Not Present

Sensor ID              : MemUnrecover Er (0x45)
 Entity ID             : 0.0
 Sensor Type (Discrete): Memory
 Unable to read sensor: Device Not Present

Sensor ID              : RCPU Diode 1 (0x46)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        :  Unable to read sensor: Device Not Present

 Event Status          : Unavailable
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr+ 

Sensor ID              : Ambient (0x47)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        : 26 (+/- 0) degrees C
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 51.000
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr+ 

Sensor ID              : Local VRD0 Temp (0x48)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        : 27 (+/- 0) degrees C
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : na
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : 

Sensor ID              : CPU Dmn 0 Temp (0x86)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        : 54 (+/- 0) degrees C
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 85.000
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr- 

Sensor ID              : Slots Amb (0x4d)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        : 33 (+/- 0) degrees C
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 85.000
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr- 

Sensor ID              : 1.8V Amb (0x4e)
 Entity ID             : 0.0
 Sensor Type (Threshold)  : Temperature
 Sensor Reading        : 46 (+/- 0) degrees C
 Status                : ok
 Lower Non-Recoverable : na
 Lower Critical        : na
 Lower Non-Critical    : na
 Upper Non-Critical    : na
 Upper Critical        : 85.000
 Upper Non-Recoverable : na
 Positive Hysteresis   : Unspecified
 Negative Hysteresis   : Unspecified
 Assertion Events      : 
 Assertions Enabled    : ucr+ 
 Deassertions Enabled  : ucr- 

Sensor ID              : Therm-Trip (0x55)
 Entity ID             : 0.0
 Sensor Type (Discrete): Processor
 States Asserted       : Digital State
                         [State Deasserted]

Sensor ID              : CPU Prochot (0x59)
 Entity ID             : 0.0
 Sensor Type (Discrete): Temperature
 States Asserted       : Digital State
                         [Limit Not Exceeded]

Sensor ID              : LOM Link Status (0x5d)
 Entity ID             : 0.0
 Sensor Type (Discrete): LAN
 States Asserted       : Digital State
                         [State Asserted]

Sensor ID              : LO100 Present (0x5e)
 Entity ID             : 0.0
 Sensor Type (Discrete): Add-in Card
 States Asserted       : Availability State
                         [Device Absent]

Sensor ID              : Watchdog (0xfe)
 Entity ID             : 0.0
 Sensor Type (Discrete): Watchdog2
 Unable to read sensor: Device Not Present

