Generating detailed summary of the adapter, it may take a while to complete.

Controller = 0
Status = Success
Description = None


Basics :
======
Controller = 0
Model = LSI 2108 MegaRAID
Serial Number = FW-ABCDEFGHIJKLM
Current Controller Date/Time = 12/24/2022, 10:33:04
Current System Date/time = 12/24/2022, 10:33:22
SAS Address = 5003048014579200
PCI Address = 00:82:00:00
Mfg Date = 00/00/00
Rework Date = 00/00/00
Revision No = 


Version :
=======
Firmware Package Build = 12.15.0-0239
Firmware Version = 2.130.403-4660
Bios Version = 3.30.02.2_4.16.08.00_0x06060A05
Preboot CLI Version = 04.04-020:#%00009
WebBIOS Version = 6.0-54-e_50-Rel
NVDATA Version = 2.09.03-0058
Boot Block Version = 2.02.00.00-0000
Bootloader Version = 09.250.01.219
Driver Name = megaraid_sas
Driver Version = 07.717.02.00-rc1


Bus :
===
Vendor Id = 0x1000
Device Id = 0x79
SubVendor Id = 0x15D9
SubDevice Id = 0x700
Host Interface = PCI-E
Device Interface = SAS-6G
Bus Number = 130
Device Number = 0
Function Number = 0


Pending Images in Flash :
=======================
Image name = No pending images


Status :
======
Controller Status = Optimal
Memory Correctable Errors = 0
Memory Uncorrectable Errors = 0
ECC Bucket Count = 0
Any Offline VD Cache Preserved = No
BBU Status = 44
Support PD Firmware Download = No
Lock Key Assigned = No
Failed to get lock key on bootup = No
Lock key has not been backed up = No
Bios was not detected during boot = No
Controller must be rebooted to complete security operation = No
A rollback operation is in progress = No
At least one PFK exists in NVRAM = No
SSC Policy is WB = No
Controller has booted into safe mode = No


Supported Adapter Operations :
============================
Rebuild Rate = Yes
CC Rate = Yes
BGI Rate  = Yes
Reconstruct Rate = Yes
Patrol Read Rate = Yes
Alarm Control = Yes
Cluster Support = No
BBU  = Yes
Spanning = Yes
Dedicated Hot Spare = Yes
Revertible Hot Spares = Yes
Foreign Config Import = Yes
Self Diagnostic = Yes
Allow Mixed Redundancy on Array = No
Global Hot Spares = Yes
Deny SCSI Passthrough = No
Deny SMP Passthrough = No
Deny STP Passthrough = No
Support more than 8 Phys = Yes
FW and Event Time in GMT = No
Support Enhanced Foreign Import = Yes
Support Enclosure Enumeration = Yes
Support Allowed Operations = Yes
Abort CC on Error = Yes
Support Multipath = Yes
Support Odd & Even Drive count in RAID1E = No
Support Security = No
Support Config Page Model = Yes
Support the OCE without adding drives = Yes
Support EKM = No
Snapshot Enabled = No
Support PFK = Yes
Support PI = No
Support Ld BBM Info = No
Support Shield State = No
Block SSD Write Disk Cache Change = No
Support Suspend Resume BG ops = No
Support Emergency Spares = Yes
Support Set Link Speed = No
Support Boot Time PFK Change = No
Support JBOD = No
Disable Online PFK Change = No
Support Perf Tuning = No
Support SSD PatrolRead = Yes
Real Time Scheduler = Yes
Support Reset Now = Yes
Support Emulated Drives = Yes
Headless Mode = Yes
Dedicated HotSpares Limited = No
Point In Time Progress = No
Extended LD = No
Boot Volume Supported = No
Support Uneven span  = No
Support Config Auto Balance = No
Support Maintenance Mode = No
Support Diagnostic results = No
Support Ext Enclosure = No
Support Sesmonitoring = No
Support SecurityonJBOD = No
Support ForceFlash = No
Support DisableImmediateIO = Yes
Support LargeIOSupport = No
Support DrvActivityLEDSetting = Yes
Support FlushWriteVerify = No
Support CPLDUpdate = No
Support ForceTo512e = No
Support discardCacheDuringLDDelete = No
Support JBOD Write cache = No
Support Large QD Support = No
Support SRIOV Options = No


Supported PD Operations :
=======================
Force Online = Yes
Force Offline = Yes
Force Rebuild = Yes
Deny Force Failed = No
Deny Force Good/Bad = No
Deny Missing Replace = No
Deny Clear = No
Deny Locate = No
Support Power State = Yes
Set Power State For Cfg = No
Support T10 Power State = No
Support Temperature = Yes
NCQ = No
Support Max Rate SATA = No
Support Degraded Media = No
Support Parallel FW Update = No
Support Drive Crypto Erase = No


Supported VD Operations :
=======================
Read Policy = Yes
Write Policy = Yes
IO Policy = Yes
Access Policy = Yes
Disk Cache Policy = Yes
Reconstruction = Yes
Deny Locate = No
Deny CC = No
Allow Ctrl Encryption = No
Enable LDBBM = Yes
Support FastPath = No
Performance Metrics = Yes
Power Savings = No
Support Powersave Max With Cache = No
Support Breakmirror = No
Support SSC WriteBack = No
Support SSC Association = Yes
Support VD Hide = No
Support VD Cachebypass = No
Support VD discardCacheDuringLDDelete = No


Advanced Software Option :
========================

-------------------------------------
Adv S/W Opt     Time Remaining  Mode 
-------------------------------------
MegaRAID RAID6  Unlimited       -    
MegaRAID RAID5  Unlimited       -    
-------------------------------------

Safe ID =  JJ17M5BUPUQ81RDKM9HGF7IMB81U6ME2RUI7432Z

HwCfg :
=====
ChipRevision =  B4
BatteryFRU = N/A
Front End Port Count = 0
Backend Port Count = 8
BBU = Present
Alarm = On
Serial Debugger = Present
NVRAM Size = 32KB
Flash Size = 8MB
On Board Memory Size = 512MB
CacheVault Flash Size = NA
TPM = Absent
Upgrade Key = Absent
On Board Expander = Absent
Temperature Sensor for ROC = Absent
Temperature Sensor for Controller = Absent
Upgradable CPLD = Absent
Current Size of CacheCade (GB) = 0
Current Size of FW Cache (MB) = 346


Policies :
========

Policies Table :
==============

------------------------------------------------
Policy                          Current Default 
------------------------------------------------
Predictive Fail Poll Interval   300 sec         
Interrupt Throttle Active Count 16              
Interrupt Throttle Completion   50 us           
Rebuild Rate                    30 %    30%     
PR Rate                         30 %    30%     
BGI Rate                        30 %    30%     
Check Consistency Rate          30 %    30%     
Reconstruction Rate             30 %    30%     
Cache Flush Interval            4s              
------------------------------------------------

Flush Time(Default) = 4s
Drive Coercion Mode = 1GB
Auto Rebuild = On
Battery Warning = On
ECC Bucket Size = 15
ECC Bucket Leak Rate (hrs) = 24
Restore HotSpare on Insertion = Off
Expose Enclosure Devices = On
Maintain PD Fail History = Off
Reorder Host Requests = On
Auto detect BackPlane = SGPIO/i2c SEP
Load Balance Mode = Auto
Security Key Assigned = Off
Disable Online Controller Reset = Off
Use drive activity for locate = Off


Boot :
====
BIOS Enumerate VDs = 1
Stop BIOS on Error = On
Delay during POST = 0
Spin Down Mode = None
Enable Ctrl-R = No
Enable Web BIOS = Yes
Enable PreBoot CLI = Yes
Enable BIOS = Yes
Max Drives to Spinup at One Time = 4
Maximum number of direct attached drives to spin up in 1 min = 120
Delay Among Spinup Groups (sec) = 2
Allow Boot with Preserved Cache = Off


High Availability :
=================
Topology Type = None
Cluster Permitted = No
Cluster Active = No


Defaults :
========
Phy Polarity = 0
Phy PolaritySplit = 0
Strip Size = 64 KB
Write Policy = WB
Read Policy = Adaptive
Cache When BBU Bad = On
Cached IO = On
VD PowerSave Policy = Controller Defined
Default spin down time (mins) = 30
Coercion Mode = 1 GB
ZCR Config = Unknown
Max Chained Enclosures = 16
Direct PD Mapping = Yes
Restore Hot Spare on Insertion = No
Expose Enclosure Devices = Yes
Maintain PD Fail History = No
Zero Based Enclosure Enumeration = No
Disable Puncturing = No
EnableLDBBM = Yes
DisableHII = No
Un-Certified Hard Disk Drives = Allow
SMART Mode = Mode 6
Enable LED Header = No
LED Show Drive Activity = Yes
Dirty LED Shows Drive Activity = No
EnableCrashDump = No
Disable Online Controller Reset = No
Treat Single span R1E as R10 = No
Power Saving option = Enabled
TTY Log In Flash = No
Auto Enhanced Import = No
BreakMirror RAID Support = No
Disable Join Mirror = No
Enable Shield State = No
Time taken to detect CME = 60 sec


Capabilities :
============
Supported Drives = SAS, SATA
Boot Volume Supported = NO
RAID Level Supported = RAID0, RAID1, RAID5, RAID6, RAID00, RAID10, RAID50, 
RAID60, PRL 11, PRL 11 with spanning, SRL 3 supported, 
PRL11-RLQ0 DDF layout with no span, PRL11-RLQ0 DDF layout with span
Enable JBOD = No
Mix in Enclosure = Allowed
Mix of SAS/SATA of HDD type in VD = Allowed
Mix of SAS/SATA of SSD type in VD = Allowed
Mix of SSD/HDD in VD = Allowed
SAS Disable = No
Max Arms Per VD = 32
Max Spans Per VD = 8
Max Arrays = 128
Max VD per array = 16
Max Number of VDs = 64
Max Parallel Commands = 1008
Max SGE Count = 80
Max Data Transfer Size = 8192 sectors
Max Strips PerIO = 42
Max Configurable CacheCade Size(GB) = 0
Max Transportable DGs = 0
Min Strip Size = 8 KB
Max Strip Size = 1.0 MB


Scheduled Tasks :
===============
Consistency Check Reoccurrence = 672 hrs
Next Consistency check launch = 12/24/2022, 04:00:00
Patrol Read Reoccurrence = 672 hrs
Next Patrol Read launch = 12/25/2022, 04:00:00
Battery learn Reoccurrence = 672 hrs
Next Battery Learn = 12/24/2022, 04:00:00
OEMID = LSI

Drive Groups = 1

TOPOLOGY :
========

----------------------------------------------------------------------------
DG Arr Row EID:Slot DID Type  State BT      Size PDC  PI SED DS3  FSpace TR 
----------------------------------------------------------------------------
 0 -   -   -        -   RAID5 Optl  Y  10.913 TB dflt N  N   none N      N  
 0 0   -   -        -   RAID5 Optl  Y  10.913 TB dflt N  N   none N      N  
 0 0   0   252:0    0   DRIVE Onln  N   2.727 TB dflt N  N   none -      N  
 0 0   1   252:1    1   DRIVE Onln  N   2.727 TB dflt N  N   none -      N  
 0 0   2   252:2    2   DRIVE Onln  N   2.727 TB dflt N  N   none -      N  
 0 0   3   252:3    3   DRIVE Onln  N   2.727 TB dflt N  N   none -      N  
 0 0   4   252:4    4   DRIVE Onln  N   2.727 TB dflt N  N   none -      N  
----------------------------------------------------------------------------

DG=Disk Group Index|Arr=Array Index|Row=Row Index|EID=Enclosure Device ID
DID=Device ID|Type=Drive Type|Onln=Online|Rbld=Rebuild|Dgrd=Degraded
Pdgd=Partially degraded|Offln=Offline|BT=Background Task Active
PDC=PD Cache|PI=Protection Info|SED=Self Encrypting Drive|Frgn=Foreign
DS3=Dimmer Switch 3|dflt=Default|Msng=Missing|FSpace=Free Space Present
TR=Transport Ready

Virtual Drives = 1

VD LIST :
=======

--------------------------------------------------------------
DG/VD TYPE  State Access Consist Cache Cac sCC      Size Name 
--------------------------------------------------------------
0/0   RAID5 Optl  RW     Yes     RWBC  -   ON  10.913 TB      
--------------------------------------------------------------

Cac=CacheCade|Rec=Recovery|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
AWB=Always WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency

Physical Drives = 5

PD LIST :
=======

-----------------------------------------------------------------------------------
EID:Slt DID State DG     Size Intf Med SED PI SeSz Model                   Sp Type 
-----------------------------------------------------------------------------------
252:0     0 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:1     1 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:2     2 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:3     3 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:4     4 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
-----------------------------------------------------------------------------------

EID-Enclosure Device ID|Slt-Slot No.|DID-Device ID|DG-DriveGroup
DHS-Dedicated Hot Spare|UGood-Unconfigured Good|GHS-Global Hotspare
UBad-Unconfigured Bad|Onln-Online|Offln-Offline|Intf-Interface
Med-Media Type|SED-Self Encryptive Drive|PI-Protection Info
SeSz-Sector Size|Sp-Spun|U-Up|D-Down|T-Transition|F-Foreign
UGUnsp-Unsupported|UGShld-UnConfigured shielded|HSPShld-Hotspare shielded
CFShld-Configured shielded|Cpybck-CopyBack|CBShld-Copyback Shielded


BBU_Info :
========

-----------------------------------------------------------------------
Model  State   RetentionTime Temp Mode MfgDate    Next Learn           
-----------------------------------------------------------------------
iBBU08 Optimal 48 hours +    47C  1    2012/08/22 2022/13/24  04:00:00 
-----------------------------------------------------------------------

Mode 1: 12+ Hrs retention with a transparent learn cycle 
           and best service life.

Controller = 0
Status = Success
Description = None


/c0/v0 :
======

--------------------------------------------------------------
DG/VD TYPE  State Access Consist Cache Cac sCC      Size Name 
--------------------------------------------------------------
0/0   RAID5 Optl  RW     Yes     RWBC  -   ON  10.913 TB      
--------------------------------------------------------------

Cac=CacheCade|Rec=Recovery|OfLn=OffLine|Pdgd=Partially Degraded|Dgrd=Degraded
Optl=Optimal|RO=Read Only|RW=Read Write|HD=Hidden|TRANS=TransportReady|B=Blocked|
Consist=Consistent|R=Read Ahead Always|NR=No Read Ahead|WB=WriteBack|
AWB=Always WriteBack|WT=WriteThrough|C=Cached IO|D=Direct IO|sCC=Scheduled
Check Consistency


PDs for VD 0 :
============

-----------------------------------------------------------------------------------
EID:Slt DID State DG     Size Intf Med SED PI SeSz Model                   Sp Type 
-----------------------------------------------------------------------------------
252:0     0 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:1     1 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:2     2 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:3     3 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
252:4     4 Onln   0 2.727 TB SATA HDD N   N  512B Hitachi HUA723030ALA641 U  -    
-----------------------------------------------------------------------------------

EID-Enclosure Device ID|Slt-Slot No.|DID-Device ID|DG-DriveGroup
DHS-Dedicated Hot Spare|UGood-Unconfigured Good|GHS-Global Hotspare
UBad-Unconfigured Bad|Onln-Online|Offln-Offline|Intf-Interface
Med-Media Type|SED-Self Encryptive Drive|PI-Protection Info
SeSz-Sector Size|Sp-Spun|U-Up|D-Down|T-Transition|F-Foreign
UGUnsp-Unsupported|UGShld-UnConfigured shielded|HSPShld-Hotspare shielded
CFShld-Configured shielded|Cpybck-CopyBack|CBShld-Copyback Shielded


VD0 Properties :
==============
Strip Size = 64 KB
Number of Blocks = 23437492224
VD has Emulated PD = No
Span Depth = 1
Number of Drives Per Span = 5
Write Cache(initial setting) = WriteBack
Disk Cache Policy = Disk's Default
Encryption = None
Data Protection = None
Active Operations = Consistency Check (95%)
Exposed to OS = Yes
Creation Date = 29-04-2021
Creation Time = 10:53:28 AM
Emulation type = default
Is LD Ready for OS Requests = Yes
SCSI NAA Id = 6003048014579200281d4ca843bb0950


