==============NVSMI LOG==============

Timestamp : Thu Aug 11 22:42:34 2016
Driver Version : 352.93

Attached GPUs : 2
GPU 0000:05:00.0
    Product Name : Tesla K80
    Product Brand : Tesla
    Display Mode : Disabled
    Display Active : Disabled
    Persistence Mode : Disabled
    Accounting Mode : Disabled
    Accounting Mode Buffer Size : 1920
    Driver Model
        Current : N/A
        Pending : N/A
    Serial Number : 0325515512345
    GPU UUID : GPU-a65eaaaa-8871-ded5-b6ee-526840412345
    Minor Number : 0
    VBIOS Version : 80.21.1B.00.01
    MultiGPU Board : Yes
    Board ID : 0x300
    Inforom Version
        Image Version : 2080.0200.00.04
        OEM Object : 1.1
        ECC Object : 3.0
        Power Management Object : N/A
    GPU Operation Mode
        Current : N/A
        Pending : N/A
    PCI
        Bus : 0x05
        Device : 0x00
        Domain : 0x0000
        Device Id : 0x102D10DE
        Bus Id : 0000:05:00.0
        Sub System Id : 0x106C10DE
        GPU Link Info
            PCIe Generation
                Max : 3
                Current : 3
            Link Width
                Max : 16x
                Current : 16x
        Bridge Chip
            Type : PLX
            Firmware : 0xF0472900
        Replays since reset : 0
        Tx Throughput : N/A
        Rx Throughput : N/A
    Fan Speed : N/A
    Performance State : P0
    Clocks Throttle Reasons
        Idle : Not Active
        Applications Clocks Setting : Active
        SW Power Cap : Not Active
        HW Slowdown : Not Active
        Unknown : Not Active
    FB Memory Usage
        Total : 12287 MiB
        Used : 56 MiB
        Free : 12231 MiB
    BAR1 Memory Usage
        Total : 16384 MiB
        Used : 2 MiB
        Free : 16382 MiB
    Compute Mode : Default
    Utilization
        Gpu : 0 %
        Memory : 0 %
        Encoder : 0 %
        Decoder : 0 %
    Ecc Mode
        Current : Disabled
        Pending : Disabled
    ECC Errors
        Volatile
            Single Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
            Double Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
        Aggregate
            Single Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
            Double Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
    Retired Pages
        Single Bit ECC : 0
        Double Bit ECC : 0
        Pending : No
    Temperature
        GPU Current Temp : 31 C
        GPU Shutdown Temp : 93 C
        GPU Slowdown Temp : 88 C
    Power Readings
        Power Management : Supported
        Power Draw : 59.20 W
        Power Limit : 149.00 W
        Default Power Limit : 149.00 W
        Enforced Power Limit : 149.00 W
        Min Power Limit : 100.00 W
        Max Power Limit : 175.00 W
    Clocks
        Graphics : 562 MHz
        SM : 562 MHz
        Memory : 2505 MHz
    Applications Clocks
        Graphics : 562 MHz
        Memory : 2505 MHz
    Default Applications Clocks
        Graphics : 562 MHz
        Memory : 2505 MHz
    Max Clocks
        Graphics : 875 MHz
        SM : 875 MHz
        Memory : 2505 MHz
    Clock Policy
        Auto Boost : On
        Auto Boost Default : On
    Processes : None

GPU 0000:06:00.0
    Product Name : Tesla K80
    Product Brand : Tesla
    Display Mode : Disabled
    Display Active : Disabled
    Persistence Mode : Disabled
    Accounting Mode : Disabled
    Accounting Mode Buffer Size : 1920
    Driver Model
        Current : N/A
        Pending : N/A
    Serial Number : 0325515512346
    GPU UUID : GPU-21c2bbbb-72a9-1b68-adab-459d05d12345
    Minor Number : 1
    VBIOS Version : 80.21.1B.00.02
    MultiGPU Board : Yes
    Board ID : 0x300
    Inforom Version
        Image Version : 2080.0200.00.04
        OEM Object : 1.1
        ECC Object : 3.0
        Power Management Object : N/A
    GPU Operation Mode
        Current : N/A
        Pending : N/A
    PCI
        Bus : 0x06
        Device : 0x00
        Domain : 0x0000
        Device Id : 0x102D10DE
        Bus Id : 0000:06:00.0
        Sub System Id : 0x106C10DE
        GPU Link Info
            PCIe Generation
                Max : 3
                Current : 3
            Link Width
                Max : 16x
                Current : 16x
        Bridge Chip
            Type : PLX
            Firmware : 0xF0472900
        Replays since reset : 0
        Tx Throughput : N/A
        Rx Throughput : N/A
    Fan Speed : N/A
    Performance State : P0
    Clocks Throttle Reasons
        Idle : Not Active
        Applications Clocks Setting : Active
        SW Power Cap : Not Active
        HW Slowdown : Not Active
        Unknown : Not Active
    FB Memory Usage
        Total : 12287 MiB
        Used : 56 MiB
        Free : 12231 MiB
    BAR1 Memory Usage
        Total : 16384 MiB
        Used : 2 MiB
        Free : 16382 MiB
    Compute Mode : Default
    Utilization
        Gpu : 0 %
        Memory : 0 %
        Encoder : 0 %
        Decoder : 0 %
    Ecc Mode
        Current : Disabled
        Pending : Disabled
    ECC Errors
        Volatile
            Single Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
            Double Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
        Aggregate
            Single Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
            Double Bit
                Device Memory : N/A
                Register File : N/A
                L1 Cache : N/A
                L2 Cache : N/A
                Texture Memory : N/A
                Total : N/A
    Retired Pages
        Single Bit ECC : 0
        Double Bit ECC : 0
        Pending : No
    Temperature
        GPU Current Temp : 24 C
        GPU Shutdown Temp : 93 C
        GPU Slowdown Temp : 88 C
    Power Readings
        Power Management : Supported
        Power Draw : 70.89 W
        Power Limit : 149.00 W
        Default Power Limit : 149.00 W
        Enforced Power Limit : 149.00 W
        Min Power Limit : 100.00 W
        Max Power Limit : 175.00 W
    Clocks
        Graphics : 562 MHz
        SM : 562 MHz
        Memory : 2505 MHz
    Applications Clocks
        Graphics : 562 MHz
        Memory : 2505 MHz
    Default Applications Clocks
        Graphics : 562 MHz
        Memory : 2505 MHz
    Max Clocks
        Graphics : 875 MHz
        SM : 875 MHz
        Memory : 2505 MHz
    Clock Policy
        Auto Boost : On
        Auto Boost Default : On
    Processes : None
